Here is a complete breakdown of the most common tint technologies:

1

### Dyed Film (Entry-Level)

Cheapest
Basic look & privacy
Fades over time
Low heat rejection
Turns purple in sunlight

This type is common in low-cost shops and "$99 tint jobs."

2

### Metalized Film

Better heat rejection than dyed
Durable
Can interfere with electronics, GPS, sensors
Reflective "mirror-like" look

Rarely used in modern installations because technology has advanced far beyond this.

3

### Carbon Film

Solid heat rejection
Good longevity
Matte finish
Not as strong as ceramic
Heat rejection numbers vary by manufacturer

Carbon is considered a mid-tier modern tint option.

4

### Ceramic Film (Premium)

Excellent heat rejection
UV protection
No fading
No signal interference
Clearer visibility inside and out

Ceramic uses non-metal nano particles that block heat at a molecular level.

5

### Nano-Ceramic / IR Ceramic (Top-Tier)

Highest-performing film in the industry
Advanced IR-blocking layers
Superior clarity and color stability
Maximum comfort, especially in warm climates
Outstanding longevity

This is the gold standard in 2025 and beyond.

## Ready to Make an Informed Decision?

Whether you're planning your first tint job, comparing film types, or learning about window tinting technology—CarTinting.com provides the facts you need to choose wisely.

Start Learning National Window Tint Laws