### Why You Might Remove Tint

Upgrading to premium film

Tint is faded, bubbled, or peeling

Selling the car

1

### Steam Method

- Safest for cars with heated defrosters
- Uses steam to loosen adhesive
- Film peels off gradually

Safest Method
2

### Heat Gun / Hair Dryer Method

- Softens adhesive
- Peel film slowly
- Avoid overheating and distorting glass

Requires Care
3

### Ammonia & Plastic Bag Method

- Place a plastic bag with ammonia on the window
- Loosen adhesive over several hours
- Carefully peel film

Time-Intensive

### Safety Tips

#### Avoid scratching the glass

#### Avoid cutting or damaging defroster lines

#### Wear gloves and safety glasses

#### Clean residue thoroughly after removal

## Ready to Make an Informed Decision?

Whether you're planning your first tint job, comparing film types, or learning about window tinting technology—CarTinting.com provides the facts you need to choose wisely.

Start Learning National Window Tint Laws