1

## Factory Tint

- Installed at the manufacturer
- Usually light, cosmetic film
- Provides some privacy but minimal heat rejection
- Non-removable, cannot upgrade
- Meets basic regulatory requirements

Basic
Fixed
2

## Aftermarket Tint

- Installed by professional shops
- Choice of film type (carbon, ceramic, nano-ceramic)
- Superior heat and UV protection
- Can be customized for VLT, privacy, and performance
- Replaceable and upgradable

Premium
Customizable

### Which Is Better?

#### Factory Tint

Fine for basic privacy

#### Aftermarket Tint

Ideal for heat control, performance, and aesthetics

### Feature Comparison

Installation
Factory: Manufacturer
Aftermarket: Professional Shop
Film Type
Factory: Basic, Light Film
Aftermarket: Carbon, Ceramic, Nano-Ceramic
Heat Rejection
Factory: Minimal
Aftermarket: Superior
Customization
Factory: None
Aftermarket: Full Customization
Replaceable
Factory: No
Aftermarket: Yes

## Ready to Make an Informed Decision?

Whether you're planning your first tint job, comparing film types, or learning about window tinting technology—CarTinting.com provides the facts you need to choose wisely.

Start Learning National Window Tint Laws